RC 4-Axis Model Quadcopter Parts 30A Electronic Brushless Motor Speed Controller ESC

30A Brushless ESC Electronic Speed Controller for DJI Flame F450 Multicopter Quadcopter

Features:

Simonk firmware

With low voltage, overheat protection and self detection function

MCU and BEC with independant regulator

Parameter adjustable by programer or remote controller

Throttle stroke adjustable, compatible with different receivers.

Built-in linear BEC or switch mode BEC

Continuous current: 30A

Burst current: 40A

Linear BEC: 2A/5V

Input voltage: 6-12.6V(2-3S lipo)

Dimension: 55\*28\*7mm

Weight: 28g

BEC mode: Linear

BEC Output: 5V 2A

Max speed: 210000 rpm for 2-pole, 70000 rpm for 6-pole, 35000 rpm for 12-pole

Package list:

1 x 30A Brushless ESC Electronic Speed Controller